(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 66)
    (no_connects 2)
    (area 167.793999 74.829999 235.558001 174.588)
    (thickness 1.6)
    (drawings 12)
    (tracks 195)
    (zones 0)
    (modules 45)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.41)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 1.000000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C2-Pad1)")
  (net 2 "Net-(C2-Pad2)")
  (net 3 "Net-(C4-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D2-Pad4)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(Q3-Pad1)")
  (net 9 "Net-(C1-Pad1)")
  (net 10 "Net-(C1-Pad2)")
  (net 11 "Net-(D5-Pad2)")
  (net 12 "Net-(C3-Pad1)")
  (net 13 "Net-(C3-Pad2)")
  (net 14 "Net-(D7-Pad2)")
  (net 15 "Net-(C5-Pad1)")
  (net 16 "Net-(C7-Pad1)")
  (net 17 "Net-(C7-Pad2)")
  (net 18 "Net-(D9-Pad1)")
  (net 19 "Net-(F1-Pad2)")
  (net 20 "Net-(C8-Pad1)")
  (net 21 "Net-(D11-Pad2)")
  (net 22 "Net-(D12-Pad1)")
  (net 23 "Net-(F1-Pad1)")
  (net 24 "Net-(C5-Pad2)")
  (net 25 "Net-(R3-Pad1)")
  (net 26 "Net-(D13-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.75)
    (via_dia 0.41)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(R3-Pad1)")
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 580B4C4B)
    (at 223.266 102.108)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R13 (at 6.096 2.286 180) (layer F.SilkS))
    (fp_text value 1meg (at 4.064 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(C7-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57F85BA1)
    (at 228.346 129.032 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 2.032 -2.54 180) (layer F.SilkS))
    (fp_text value 1K (at 4.064 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 25 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C4-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57F855B6)
    (at 200.406 135.636 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 4.572 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 2.032 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 580B47CC)
    (at 220.472 124.714)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at -2.286 0.254 180) (layer F.SilkS))
    (fp_text value 2uf (at 5.08 -1.524 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.00mm (layer F.Cu) (tedit 57EDD347)
    (at 180.594 140.208 180)
    (descr "Through hole pin header, 1x04, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference D2 (at 0 8.89 180) (layer F.SilkS))
    (fp_text value Diode_Bridge (at 6.604 2.286 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 0 2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 3 thru_hole circle (at 0 4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at 0 6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Transformers_SMPS_ThroughHole:Coilcraft-Q4434-B_Rhombus-T1311 (layer F.Cu) (tedit 57EDD241)
    (at 185.166 119.126)
    (descr "Transformator, Transformer, Flyback, Coilcraft Q4434-B, Rgombus T1311,")
    (tags "Transformator, Transformer, Flyback, Coilcraft Q4434-B, Rgombus T1311,")
    (fp_text reference T2 (at 0 -13.97) (layer F.SilkS))
    (fp_text value TRANSFO (at 2.794 9.144) (layer F.Fab))
    (fp_text user 8 (at -8.89 -10.414) (layer F.SilkS))
    (fp_text user 7 (at -3.81 -10.414) (layer F.SilkS))
    (fp_text user 2 (at -3.556 9.144) (layer F.SilkS))
    (fp_text user 1 (at -7.874 9.144) (layer F.SilkS))
    (pad 5 thru_hole circle (at 7.62 -7.62) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 2.54 -7.62) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -2.54 -7.62) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -7.62 -7.62) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -6.35 6.35) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 6.35) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D2-Pad4)"))
    (pad 3 thru_hole circle (at 2.54 6.35) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 7.62 6.35) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57F6E244)
    (at 194.056 139.446 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 6.35 -2.286 180) (layer F.SilkS))
    (fp_text value 330K (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C2-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57F855BA)
    (at 197.358 143.256 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value 100K (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(C2-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57EDD05E)
    (at 207.01 143.764 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 1.778 2.54 180) (layer F.SilkS))
    (fp_text value 100K (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D3-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57F856F0)
    (at 207.01 146.812 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at 0 -2.54 360) (layer F.SilkS))
    (fp_text value 330K (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(C3-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57F4601B)
    (at 188.722 161.036)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -3.048 0.508) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 1.016 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C3-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57F46032)
    (at 182.626 161.036)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -3.048 0) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -4.064) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57F46015)
    (at 176.022 161.036)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -3.048 0) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.016 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 580B49EC)
    (at 224.79 160.528)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 2.794 -1.016) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -4.318 0.762) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C5-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 57F85BB7)
    (at 202.438 155.956 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 2.54 -3.556 360) (layer F.SilkS))
    (fp_text value 2N4401 (at 4.064 3.048 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C3-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(Q3-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 580B4828)
    (at 213.36 129.032)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D1 (at -0.254 -4.064) (layer F.SilkS))
    (fp_text value 1N4148 (at 1.016 -2.286) (layer F.Fab))
    (fp_text user A (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L13_P3.8 (layer F.Cu) (tedit 580B47FF)
    (at 219.202 135.128)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 13mm, Pitch 3.8mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C6 (at 0.508 -2.54) (layer F.SilkS))
    (fp_text value 47uf (at 3.302 -1.524) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 3.8 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L13_P3.8.wrl
      (at (xyz 0.0748031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 580B4846)
    (at 209.042 132.08 180)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.05 -2 180) (layer F.Fab))
    (fp_text user A (at 2.794 1.651 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57F8583F)
    (at 189.738 154.432)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R8 (at -2.032 -0.508) (layer F.SilkS))
    (fp_text value 1K (at 3.556 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 "Net-(D7-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(Q3-Pad1)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 580B4838)
    (at 209.296 128.524 90)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D4 (at 6.858 -2.54 180) (layer F.SilkS))
    (fp_text value "zener 1N4733" (at 5.08 -3.81 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 270) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L13_P3.8 (layer F.Cu) (tedit 57F6E23D)
    (at 187.706 136.144 270)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 13mm, Pitch 3.8mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -3.048 3.048 360) (layer F.SilkS))
    (fp_text value 220uf (at 2.54 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 3.8 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L13_P3.8.wrl
      (at (xyz 0.0748031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57F3F5E4)
    (at 197.866 127.508 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R9 (at 10.16 0 180) (layer F.SilkS))
    (fp_text value 10K (at 3.556 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(C1-Pad2)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 580B48D2)
    (at 200.406 139.192 270)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D5 (at 3.556 -2.032 360) (layer F.SilkS))
    (fp_text value 1N4148 (at -0.508 -2.032 270) (layer F.Fab))
    (fp_text user A (at -1.778 0 360) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C2-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 57F85750)
    (at 215.646 136.144 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 4.572 -3.556 360) (layer F.SilkS))
    (fp_text value "2N4401 npn" (at 2.032 -2.032 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C6-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57F858AE)
    (at 193.802 151.384 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R10 (at 7.112 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at 3.556 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C1-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L13_P3.8 (layer F.Cu) (tedit 580B458B)
    (at 215.138 155.956 90)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 13mm, Pitch 3.8mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 7.112 -1.016 180) (layer F.SilkS))
    (fp_text value 10uf (at 2.54 -2.032 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 3.8 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C3-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L13_P3.8.wrl
      (at (xyz 0.0748031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 57F85715)
    (at 210.058 157.988 180)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D6 (at -2.54 -0.508 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.05 -2 180) (layer F.Fab))
    (fp_text user A (at 2.794 1.651 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C3-Pad2)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 57F85598)
    (at 189.738 147.32 270)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D7 (at -1.016 3.048 360) (layer F.SilkS))
    (fp_text value 1N4148 (at 3.048 2.032 270) (layer F.Fab))
    (fp_text user A (at 2.794 1.651 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 580B490B)
    (at 197.358 147.574)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 5.334 -2.54 180) (layer F.SilkS))
    (fp_text value 2N4403 (at 0.762 3.048) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D5-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L13_P3.8 (layer F.Cu) (tedit 580B4584)
    (at 224.79 155.448 90)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 13mm, Pitch 3.8mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C5 (at 1.9 -5.3 90) (layer F.SilkS))
    (fp_text value 4.7uf (at 2.54 -1.778 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 3.8 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C5-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L13_P3.8.wrl
      (at (xyz 0.0748031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L13_P3.8 (layer F.Cu) (tedit 57FEE817)
    (at 202.946 97.028 270)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 13mm, Pitch 3.8mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C7 (at 1.9 -5.3 270) (layer F.SilkS))
    (fp_text value 47uf (at 7.62 0 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 3.8 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C7-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L13_P3.8.wrl
      (at (xyz 0.0748031 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 580B47C0)
    (at 219.202 120.904)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D8 (at -2.54 -0.508) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.54 -3.81) (layer F.Fab))
    (fp_text user A (at -2.032 1.27) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C4-Pad1)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 580B4D4E)
    (at 218.694 90.932 180)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D9 (at -2.54 1.27 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 2.794 -2.286 180) (layer F.Fab))
    (fp_text user A (at 2.794 1.651 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D9-Pad1)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 552FFCCE)
    (at 212.598 95.504 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D10 (at 5.38734 2.53746 270) (layer F.SilkS))
    (fp_text value "7v zener" (at 4.37134 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C7-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C7-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 580B4B87)
    (at 219.71 95.504)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R11 (at 1.778 -2.54) (layer F.SilkS))
    (fp_text value 2200 (at 4.064 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(D9-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 580B4B8D)
    (at 233.68 90.932 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R12 (at 1.27 -2.54 180) (layer F.SilkS))
    (fp_text value 1meg (at 3.556 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 "Net-(D12-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(C8-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_B3S-1000 (layer F.Cu) (tedit 56EDA1C6)
    (at 205.486 88.9)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value SPST (at 0 4.5) (layer F.Fab))
    (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(F1-Pad2)"))
    (pad 1 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(F1-Pad2)"))
    (pad 2 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D11-Pad2)"))
  )
  (module Transformers_SMPS_ThroughHole:Coilcraft-Q4434-B_Rhombus-T1311 (layer F.Cu) (tedit 580B4B2D)
    (at 186.69 92.964 90)
    (descr "Transformator, Transformer, Flyback, Coilcraft Q4434-B, Rgombus T1311,")
    (tags "Transformator, Transformer, Flyback, Coilcraft Q4434-B, Rgombus T1311,")
    (fp_text reference T1 (at 0 -13.97 90) (layer F.SilkS))
    (fp_text value TRANSFO (at 4.826 2.032 180) (layer F.Fab))
    (fp_text user 8 (at -8.89 -10.414 90) (layer F.SilkS))
    (fp_text user 7 (at -3.81 -10.414 90) (layer F.SilkS))
    (fp_text user 2 (at -3.556 9.144 90) (layer F.SilkS))
    (fp_text user 1 (at -7.874 9.144 90) (layer F.SilkS))
    (pad 5 thru_hole circle (at 7.62 -7.62 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 2.54 -7.62 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -2.54 -7.62 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -7.62 -7.62 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -6.35 6.35 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -2.54 6.35 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 2.54 6.35 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C7-Pad2)"))
    (pad 4 thru_hole circle (at 7.62 6.35 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(F1-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 580B4B97)
    (at 230.886 96.52 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -1.524 -2.032 360) (layer F.SilkS))
    (fp_text value 0.001uf (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C7-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Vertical_AnodeUp (layer F.Cu) (tedit 580B4D55)
    (at 221.234 85.598 180)
    (descr "Diode, DO-41, SOD81, Vertical, Anode Up,")
    (tags "Diode, DO-41, SOD81, Vertical, Anode Up, 1N4007, SB140,")
    (fp_text reference D11 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.05 -2 180) (layer F.Fab))
    (fp_text user A (at 2.794 1.651 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C8-Pad1)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 552FFCCE)
    (at 226.822 105.918 180)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D12 (at 5.38734 2.53746 180) (layer F.SilkS))
    (fp_text value "7v zener" (at 4.37134 -3.55854 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C7-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D12-Pad1)"))
  )
  (module Fuse_Holders_and_Fuses:BladeFuse-CarType (layer F.Cu) (tedit 580B4E51)
    (at 213.614 80.264)
    (fp_text reference F1 (at 0 -4.064) (layer F.SilkS))
    (fp_text value FUSEA (at 12.446 0.254) (layer F.Fab))
    (pad 1 thru_hole oval (at -4.65 0) (size 8 3.8) (drill oval 6 2) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(F1-Pad1)"))
    (pad 2 thru_hole oval (at 4.65 0) (size 8 3.8) (drill oval 6 2) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(F1-Pad2)"))
    (model Fuse_Holders_and_Fuses.3dshapes/BladeFuse-CarType.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistors:RV_Disc_D7_W3.4_P5 (layer F.Cu) (tedit 580B47E8)
    (at 227.076 146.558 90)
    (tags "varistor SIOV")
    (fp_text reference VR1 (at 2.54 0.762 90) (layer F.SilkS))
    (fp_text value "rheostat 1K" (at -6.35 2.286 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 5 1.3 90) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R3-Pad1)"))
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 580B4819)
    (at 223.012 141.732 270)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D13 (at 6.604 -0.254 360) (layer F.SilkS))
    (fp_text value LED (at 5.08 -0.254 360) (layer F.Fab))
    (fp_text user K (at -2.286 -1.778 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(D13-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 580B481F)
    (at 219.202 148.336 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R14 (at 4.572 -2.286 90) (layer F.SilkS))
    (fp_text value 1K (at 4.064 0.254 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 12 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 "Net-(D13-Pad2)"))
  )
  (gr_text "Receiver Data Input" (at 221.234 163.83) (layer F.Cu))
  (gr_text "Your AC Load\n\n" (at 186.182 165.1) (layer F.Cu))
  (gr_text "Transmitter power supply\nand 60 Hz data supply" (at 188.722 79.756) (layer F.Cu))
  (gr_text "315Mhz remote switch receiver/transmitter\nfeaturing: press 1s for ON, press 3s for OFF.\nKiCAD 4.03" (at 178.816 170.688) (layer F.Cu))
  (gr_text "315Mhz receiver latch\nswitches AC load off/on" (at 207.01 113.792) (layer F.Cu))
  (gr_text "60Hz pulse data goes into P4/gnd from receiver (1s or 3s of pulses)" (at 230.886 142.494 90) (layer F.Cu))
  (gr_text "9vac \npower supply" (at 175.768 117.094) (layer F.Cu))
)
